<?xml version="1.0" encoding="utf-8"?>
<SCL xmlns="http://www.iec.ch/61850/2003/SCL" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
  <Header id="" nameStructure="IEDName"/>
  <Communication>
    <SubNetwork name="RZANW" desc="8-MMS" type="8-MMS">
      <ConnectedAP apName="S1" iedName="RZANW">
        <Address>
          <P type="IP" xsi:type="tP_IP">0.0.0.0</P>
        </Address>
        <GSE ldInst="C1" cbName="Goose1">
          <Address>
            <P type="MAC-Address">01-0C-CD-01-00-01</P>
            <P type="APPID">3001</P>
            <P type="VLAN-PRIORITY">5</P>
            <P type="MinTime">2</P>
            <P type="MaxTime">100</P>
          </Address>
        </GSE>
      </ConnectedAP>
    </SubNetwork>
  </Communication>
  <IED name="IEDname" type="IEDtype" manufacturer="Relsis" configVersion="1">
    <Services>
      <DynAssociation/>
      <GetDirectory/>
      <GetDataObjectDefinition/>
      <GetDataSetValue/>
      <DataSetDirectory/>
      <ReadWrite/>
      <GetCBValues/>
      <ConfLNs fixPrefix="true" fixLnInst="true"/>
      <ReportSettings cbName="Fix" datSet="Fix" rptID="Fix" optFields="Fix" bufTime="Fix" trgOps="Fix" intgPd="Fix"/>
      <GOOSE max="5"/>
      <GSSE max="5"/>
      <FileHandling/>
      <GSEDir/>
      <TimerActivatedControl/>
      <ConfDataSet max="5" maxAttributes="30"/>
      <ConfReportControl max="5"/>
    </Services>
    <AccessPoint name="S1">
      <Server>
        <Authentication/>
        <LDevice inst="LDeviceInst">
          <LN0 lnClass="LLN0" lnType="LLN01" inst="">
            <DOI name="Mod">
              <DAI name="ctlModel">
                <Val>status-only</Val>
              </DAI>
            </DOI>
            <DOI name="NamPlt">
              <DAI name="vendor">
                <Val>Relsis</Val>
              </DAI>
              <DAI name="swRev">
                <Val>rev1</Val>
              </DAI>
              <DAI name="d">
                <Val>d</Val>
              </DAI>
            </DOI>
            <!--DataSet-->
            <!--ReportControl-->
            <!--GSEControl-->
          </LN0>
          <LN lnClass="LPHD" lnType="LPHD1" inst="1" prefix="">
            <DOI name="Proxy">
              <DAI name="stVal">
                <Val>false</Val>
              </DAI>
            </DOI>
            <DOI name="PhyNam">
              <DAI name="vendor">
                <Val>LPHD vendor</Val>
              </DAI>
            </DOI>
          </LN>
          <LN lnType="CMSQI1" prefix="C" lnClass="MSQI" inst="1"/>
          <LN lnType="CMMXU1" prefix="C" lnClass="MMXU" inst="1"/>
          <LN lnType="VMMXU1" prefix="V" lnClass="MMXU" inst="1"/>
          <LN lnType="VNMMXU1" prefix="VN" lnClass="MMXU" inst="1"/>
          <LN lnType="VMSQI1" prefix="V" lnClass="MSQI" inst="1"/>
          <LN lnType="CVMMXU1" prefix="CV" lnClass="MMXU" inst="1"/>
          <LN lnType="CMSTA1" prefix="C" lnClass="MSTA" inst="1"/>
          <LN lnType="SP16GGIO1" prefix="SP16" lnClass="GGIO" inst="1"/>
          <LN lnType="SP16GGIO2" prefix="SP16" lnClass="GGIO" inst="2"/>
          <LN lnType="XGGIO3" prefix="X" lnClass="GGIO" inst="3"/>
          <LN lnType="LEDGGIO3" prefix="LED" lnClass="GGIO" inst="3"/>
          <LN lnType="LLED1" lnClass="LLED" inst="1"/>
          <LN lnType="CBCBCSWI1" prefix="CB" lnClass="CBCSWI" inst="1"/>
          <LN lnType="SP16GGIO5" prefix="SP16" lnClass="GGIO" inst="5"/>
          <LN lnType="SP16GGIO7" prefix="SP16" lnClass="GGIO" inst="7"/>
          <LN lnType="CBCSWI1" prefix="CB" lnClass="CSWI" inst="1"/>
          <LN lnType="PHIPTOC1" prefix="PHI" lnClass="PTOC" inst="1"/>
          <LN lnType="PHIPTOC2" prefix="PHI" lnClass="PTOC" inst="2"/>
          <LN lnType="PHIPTOC3" prefix="PHI" lnClass="PTOC" inst="3"/>
          <LN lnType="SP16GGIO8" prefix="SP16" lnClass="GGIO" inst="8"/>
        </LDevice>
      </Server>
    </AccessPoint>
  </IED>
  <DataTypeTemplates>
    <LNodeType id="LLN01" lnClass="LLN0">
      <DO name="Mod" type="INC_1_Mod"/>
      <DO name="Beh" type="INS_1_Beh"/>
      <DO name="Health" type="INS1Health"/>
      <DO name="NamPlt" type="LPL1NamPlt"/>
    </LNodeType>
    <LNodeType id="LPHD1" lnClass="LPHD">
      <DO name="PhyNam" type="DPL1PhyNam"/>
      <DO name="PhyHealth" type="INS_1_Beh"/>
      <DO name="Proxy" type="SPS1Proxy"/>
    </LNodeType>
    <LNodeType id="MMXU1" lnClass="MMXU">
      <DO name="Mod" type="INC_1_Mod"/>
      <DO name="Beh" type="INS_1_Beh"/>
      <DO name="Health" type="INS1Health"/>
      <DO name="NamPlt" type="LPL1NamPlt"/>
    </LNodeType>
    <LNodeType id="GGIO1" lnClass="GGIO">
      <DO name="Mod" type="INC_1_Mod"/>
      <DO name="Beh" type="INS_1_Beh"/>
      <DO name="Health" type="INS1Health"/>
      <DO name="NamPlt" type="LPL1NamPlt"/>
    </LNodeType>
    <LNodeType id="XCBR1" lnClass="XCBR"/>
    <LNodeType id="CMSQI1" lnClass="MSQI">
      <DO name="AAmpcVal" type="MV_TT"/>
      <DO name="VVoltcVal" type="MV_TT"/>
      <DO name="SeqAc1cVal" type="MV_TT"/>
      <DO name="SeqAc2cVal" type="MV_TT"/>
      <DO name="SeqAc3cVal" type="MV_TT"/>
      <DO name="SeqAd1cVal" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="CMMXU1" lnClass="MMXU">
      <DO name="AphsAcVal" type="MV_TT"/>
      <DO name="AphsBcVal" type="MV_TT"/>
      <DO name="AphsCcVal" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="VMMXU1" lnClass="MMXU">
      <DO name="VphsABcVal" type="MV_TT"/>
      <DO name="VphsBCcVal" type="MV_TT"/>
      <DO name="VphsCAcVal" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="VNMMXU1" lnClass="MMXU">
      <DO name="PhVphsAcVal" type="MV_TT"/>
      <DO name="PhVphsBcVal" type="MV_TT"/>
      <DO name="PhVphsCcVal" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="VMSQI1" lnClass="MSQI">
      <DO name="SeqVc2cVal" type="MV_TT"/>
      <DO name="SeqVc3cVal" type="MV_TT"/>
      <DO name="SeqVc1cVal" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="CVMMXU1" lnClass="MMXU">
      <DO name="T1mag" type="MV_TT"/>
      <DO name="T2mag" type="MV_TT"/>
      <DO name="Hzmag" type="MV_TT"/>
      <DO name="TotWmag1" type="MV_TT"/>
      <DO name="TotWmag" type="MV_TT"/>
      <DO name="TotVarmag1" type="MV_TT"/>
      <DO name="TotVarmag" type="MV_TT"/>
      <DO name="WPhsAmag" type="MV_TT"/>
      <DO name="WPhsBmag" type="MV_TT"/>
      <DO name="WPhsCmag" type="MV_TT"/>
      <DO name="VarPhsAmag" type="MV_TT"/>
      <DO name="VarPhsBmag" type="MV_TT"/>
      <DO name="VarPhsCmag" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="CMSTA1" lnClass="MSTA">
      <DO name="DH2phsAcVal" type="MV_TT"/>
      <DO name="DH2phsBcVal" type="MV_TT"/>
      <DO name="DH2phsCcVal" type="MV_TT"/>
    </LNodeType>
    <LNodeType id="SP16GGIO1" lnClass="GGIO">
      <DO name="Ind1stVal" type="SPS_TS"/>
      <DO name="Ind2stVal" type="SPS_TS"/>
      <DO name="Ind3stVal" type="SPS_TS"/>
      <DO name="Ind4stVal" type="SPS_TS"/>
      <DO name="Ind5stVal" type="SPS_TS"/>
      <DO name="Ind6stVal" type="SPS_TS"/>
      <DO name="Ind7stVal" type="SPS_TS"/>
      <DO name="Ind8stVal" type="SPS_TS"/>
      <DO name="Ind9stVal" type="SPS_TS"/>
      <DO name="Ind10stVal" type="SPS_TS"/>
      <DO name="Ind11stVal" type="SPS_TS"/>
      <DO name="Ind12stVal" type="SPS_TS"/>
      <DO name="Ind13stVal" type="SPS_TS"/>
      <DO name="Ind14stVal" type="SPS_TS"/>
      <DO name="Ind15stVal" type="SPS_TS"/>
      <DO name="Ind16stVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="SP16GGIO2" lnClass="GGIO">
      <DO name="Ind5stVal" type="SPS_TS"/>
      <DO name="Ind6stVal" type="SPS_TS"/>
      <DO name="Ind7stVal" type="SPS_TS"/>
      <DO name="Ind8stVal" type="SPS_TS"/>
      <DO name="Ind11stVal" type="SPS_TS"/>
      <DO name="Ind12stVal" type="SPS_TS"/>
      <DO name="Ind13stVal" type="SPS_TS"/>
      <DO name="Ind14stVal" type="SPS_TS"/>
      <DO name="Ind15stVal" type="SPS_TS"/>
      <DO name="Ind16stVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="XGGIO3" lnClass="GGIO">
      <DO name="SPCSO1stVal" type="SPS_TS"/>
      <DO name="SPCSO2stVal" type="SPS_TS"/>
      <DO name="SPCSO3stVal" type="SPS_TS"/>
      <DO name="SPCSO4stVal" type="SPS_TS"/>
      <DO name="SPCSO5stVal" type="SPS_TS"/>
      <DO name="SPCSO6stVal" type="SPS_TS"/>
      <DO name="SPCSO7stVal" type="SPS_TS"/>
      <DO name="SPCSO8stVal" type="SPS_TS"/>
      <DO name="SPCSO9stVal" type="SPS_TS"/>
      <DO name="SPCSO10stVal" type="SPS_TS"/>
      <DO name="SPCSO11stVal" type="SPS_TS"/>
      <DO name="SPCSO12stVal" type="SPS_TS"/>
      <DO name="SPCSO13stVal" type="SPS_TS"/>
      <DO name="SPCSO14stVal" type="SPS_TS"/>
      <DO name="SPCSO15stVal" type="SPS_TS"/>
      <DO name="SPCSO16stVal" type="SPS_TS"/>
      <DO name="SPCSO17stVal" type="SPS_TS"/>
      <DO name="SPCSO18stVal" type="SPS_TS"/>
      <DO name="SPCSO19stVal" type="SPS_TS"/>
      <DO name="SPCSO20stVal" type="SPS_TS"/>
      <DO name="SPCSO21stVal" type="SPS_TS"/>
      <DO name="SPCSO22stVal" type="SPS_TS"/>
      <DO name="SPCSO23stVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="LEDGGIO3" lnClass="GGIO">
      <DO name="Ind1stVal" type="SPS_TS"/>
      <DO name="Ind2stVal" type="SPS_TS"/>
      <DO name="Ind3stVal" type="SPS_TS"/>
      <DO name="Ind4stVal" type="SPS_TS"/>
      <DO name="Ind5stVal" type="SPS_TS"/>
      <DO name="Ind6stVal" type="SPS_TS"/>
      <DO name="Ind7stVal" type="SPS_TS"/>
      <DO name="Ind8stVal" type="SPS_TS"/>
      <DO name="Ind9stVal" type="SPS_TS"/>
      <DO name="Ind10stVal" type="SPS_TS"/>
      <DO name="Ind11stVal" type="SPS_TS"/>
      <DO name="Ind12stVal" type="SPS_TS"/>
      <DO name="Ind13stVal" type="SPS_TS"/>
      <DO name="Ind14stVal" type="SPS_TS"/>
      <DO name="Ind15stVal" type="SPS_TS"/>
      <DO name="Ind16stVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="LLED1" lnClass="LLED">
      <DO name="ONstVal" type="SPS_TS"/>
      <DO name="OFFstVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="CBCBCSWI1" lnClass="CBCSWI">
      <DO name="PosOnstVal" type="SPS_TS"/>
      <DO name="PosOnstVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="SP16GGIO5" lnClass="GGIO">
      <DO name="In1OperctlVal" type="SPS_TS"/>
      <DO name="In2OperctlVal" type="SPS_TS"/>
      <DO name="In3OperctlVal" type="SPS_TS"/>
      <DO name="In4OperctlVal" type="SPS_TS"/>
      <DO name="In5OperctlVal" type="SPS_TS"/>
      <DO name="In6OperctlVal" type="SPS_TS"/>
      <DO name="In7OperctlVal" type="SPS_TS"/>
      <DO name="In8OperctlVal" type="SPS_TS"/>
      <DO name="In9OperctlVal" type="SPS_TS"/>
      <DO name="In10OperctlVal" type="SPS_TS"/>
      <DO name="In11OperctlVal" type="SPS_TS"/>
      <DO name="In12OperctlVal" type="SPS_TS"/>
      <DO name="In13OperctlVal" type="SPS_TS"/>
      <DO name="In14.OperctlVal" type="SPS_TS"/>
      <DO name="In15.OperctlVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="SP16GGIO7" lnClass="GGIO">
      <DO name="In16OperctlVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="CBCSWI1" lnClass="CSWI">
      <DO name="PosOffstVal" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="PHIPTOC1" lnClass="PTOC">
      <DO name="Strgeneral" type="SPS_TS"/>
      <DO name="Strgeneral" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="PHIPTOC2" lnClass="PTOC">
      <DO name="Strgeneral" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="PHIPTOC3" lnClass="PTOC">
      <DO name="Strgeneral" type="SPS_TS"/>
    </LNodeType>
    <LNodeType id="SP16GGIO8" lnClass="GGIO">
      <DO name="Out1ctlVal" type="SPS_TS"/>
      <DO name="Out2ctlVal" type="SPS_TS"/>
      <DO name="Out3ctlVal" type="SPS_TS"/>
      <DO name="Out4ctlVal" type="SPS_TS"/>
      <DO name="Out5ctlVal" type="SPS_TS"/>
      <DO name="Out6ctlVal" type="SPS_TS"/>
      <DO name="Out7ctlVal" type="SPS_TS"/>
      <DO name="Out8ctlVal" type="SPS_TS"/>
      <DO name="Out9ctlVal" type="SPS_TS"/>
      <DO name="Out10ctlVal" type="SPS_TS"/>
      <DO name="Out11ctlVal" type="SPS_TS"/>
      <DO name="Out12ctlVal" type="SPS_TS"/>
      <DO name="Out13ctlVal" type="SPS_TS"/>
      <DO name="Out14ctlVal" type="SPS_TS"/>
      <DO name="Out15ctlVal" type="SPS_TS"/>
      <DO name="Out16ctlVal" type="SPS_TS"/>
    </LNodeType>
    <DOType id="INC_1_Mod" cdc="INC">
      <DA name="stVal" type="Mod" bType="Enum" fc="ST"/>
      <DA name="q" bType="Quality" fc="ST"/>
      <DA name="t" bType="Timestamp" fc="ST"/>
      <DA name="ctlModel" type="CtlModels" bType="Enum" fc="CF"/>
    </DOType>
    <DOType id="INS_1_Beh" cdc="INS">
      <DA name="stVal" type="Beh" bType="Enum" fc="ST"/>
      <DA name="q" bType="Quality" fc="ST"/>
      <DA name="t" bType="Timestamp" fc="ST"/>
    </DOType>
    <DOType id="INS1Health" cdc="INS">
      <DA name="stVal" type="Health" bType="Enum" fc="ST"/>
      <DA name="q" bType="Quality" fc="ST"/>
      <DA name="t" bType="Timestamp" fc="ST"/>
    </DOType>
    <DOType id="LPL1NamPlt" cdc="LPL">
      <DA name="vendor" bType="VisString255" fc="DC"/>
      <DA name="swRev" bType="VisString255" fc="DC"/>
      <DA name="d" bType="VisString255" fc="DC"/>
    </DOType>
    <DOType id="DPL1PhyNam" cdc="DPL">
      <DA name="vendor" bType="VisString255" fc="DC"/>
    </DOType>
    <DOType id="SPS1Proxy" cdc="SPS">
      <DA name="stVal" bType="BOOLEAN" fc="ST"/>
      <DA name="q" bType="Quality" fc="ST"/>
      <DA name="t" bType="Timestamp" fc="ST"/>
    </DOType>
    <DOType id="SPS_TS" cdc="SPS">
      <DA name="stVal" bType="BOOLEAN" fc="ST"/>
      <DA name="q" bType="Quality" fc="ST"/>
      <DA name="t" bType="Timestamp" fc="ST"/>
    </DOType>
    <DOType id="MV_TT" cdc="MV">
      <DA name="mag" type="AnalogValue1" bType="Struct" fc="MX"/>
      <DA name="q" bType="Quality" fc="MX"/>
      <DA name="t" bType="Timestamp" fc="MX"/>
    </DOType>
    <DOType id="SPC_TU" cdc="SPC">
      <DA name="stVal" bType="BOOLEAN" fc="ST"/>
      <DA name="q" bType="Quality" fc="ST"/>
      <DA name="t" bType="Timestamp" fc="ST"/>
      <DA name="Oper" bType="Struct" type="Oper_SPC" fc="CO"/>
      <DA name="ctlModel" type="CtlModels" bType="Enum" fc="CF"/>
    </DOType>
    <DOType id="ING_S" cdc="ING">
      <DA name="setVal" bType="INT16" fc="SP"/>
    </DOType>
    <DAType id="Oper_SPC">
      <BDA name="ctlVal" bType="BOOLEAN"/>
      <BDA name="origin" bType="Struct" type="Origr_SPC"/>
      <BDA name="ctlNum" bType="INT8U"/>
      <BDA name="T" bType="Timestamp"/>
      <BDA name="Test" bType="BOOLEAN"/>
      <BDA name="Check" bType="Check" type="Check"/>
    </DAType>
    <DAType id="Origr_SPC">
      <BDA name="orCat" bType="Enum" type="orCategory"/>
      <BDA name="orIdent" bType="Octet64"/>
    </DAType>
    <DAType id="AnalogValue1">
      <BDA name="f" bType="FLOAT32"/>
    </DAType>
    <EnumType id="Beh">
      <EnumVal ord="1">on</EnumVal>
      <EnumVal ord="2">blocked</EnumVal>
      <EnumVal ord="3">test</EnumVal>
      <EnumVal ord="4">test/blocked</EnumVal>
      <EnumVal ord="5">off</EnumVal>
    </EnumType>
    <EnumType id="Mod">
      <EnumVal ord="1">on</EnumVal>
      <EnumVal ord="2">blocked</EnumVal>
      <EnumVal ord="3">test</EnumVal>
      <EnumVal ord="4">test/blocked</EnumVal>
      <EnumVal ord="5">off</EnumVal>
    </EnumType>
    <EnumType id="Health">
      <EnumVal ord="1">Ok</EnumVal>
      <EnumVal ord="2">Warning</EnumVal>
      <EnumVal ord="3">Alarm</EnumVal>
    </EnumType>
    <EnumType id="CtlModels">
      <EnumVal ord="0">status-only</EnumVal>
      <EnumVal ord="1">direct-with-normal-security</EnumVal>
      <EnumVal ord="2">sbo-with-normal-security</EnumVal>
      <EnumVal ord="3">direct-with-enhanced-security</EnumVal>
      <EnumVal ord="4">sbo-with-enhanced-security</EnumVal>
    </EnumType>
    <EnumType id="orCategory">
      <EnumVal ord="0">not-supported</EnumVal>
      <EnumVal ord="1">bay-control</EnumVal>
      <EnumVal ord="2">station-control</EnumVal>
      <EnumVal ord="3">remote-control</EnumVal>
      <EnumVal ord="4">automatic-bay</EnumVal>
      <EnumVal ord="5">automatic-station</EnumVal>
      <EnumVal ord="6">automatic-remote</EnumVal>
      <EnumVal ord="7">maintenance</EnumVal>
      <EnumVal ord="8">process</EnumVal>
    </EnumType>
  </DataTypeTemplates>
</SCL>
